# System Information

This tab displays information about the license server and the system running the license server. Only users with Administrator privileges can view this page. See the following sections for an explanation about the information displayed.

| • | System Information

| • | Three-Server Redundancy Group Information

System Information

| • | Release Version: Release version of the license server.

| • | License Server Manager Port in Use: Port number that the license server manager (lmadmin) uses to listen for communication. Configure the port number in the Server Configuration tab.

| • | Display: On Windows, this is the system name or the terminal server client name (in a terminal server environment). On UNIX, this is the X-Display name or the value returned by the ttyname() (or comparable) function.

| • | Host Name: The host name of the system where the license server is running (for example, prod01).

| • | Host Domain Name: The fully qualified host name of the system on the domain where the license server is running (for example, prod01.flexerasoftware.com).

| • | IPv4 Address: IP version 4 address used to identify the system (for example, 255.255.255.255). The IPv4 address is shown when the system has IPv4 enabled. This field may appear multiple times when there are multiple addresses to display.

| • | IPv6 Address: IP version 6 address used to identify the system (for example, ffff:ffff:ffff:ffff:ffff:ffff:ffff:ffff). The IPv6 address is shown when the system has IPv6 enabled. This field may appear multiple times when there are multiple addresses to display.

| • | Ethernet Address: Ethernet address, also called hardware address or MAC address, that identifies the system where the license server is running. This field may appear multiple times when there are multiple addresses to display.

| • | Volume Serial Number: The hard disk serial number that identifies the system where the license server is running. (Displayed on systems where this hostid is available.)

| • | Flex ID: FlexNet ID dongle identity, FLEXID, that identifies a dongle attached to the license server. This field may appear multiple times when there are multiple elements to display. (Displayed on systems where this hostid is available.)

| • | Local Stop Server Allowed: Displays either yes or no. If it is no, you cannot stop the license server using the lmdown utility running on the machine where the license server is running (the local machine), nor can you stop the license server from the license server management interface. Configure this property using the –a llowStopServer command-line argument when you run the license server manager (lmadmin).

| • | Remote Stop Server Allowed: Displays either yes or no.

If it is no, you cannot stop the license server from a remote machine using lmdown or the license server management interface.

If it is yes, then you can stop the license server using either of the following:

| • | lmdown from a machine other than that where lmadmin is running (a remote machine).

| • | Stop Server button on a license server management interface that is running on a remote machine.

| • | License Reclaim Allowed: Displays either yes or no. If it is no, you cannot use the lmremove utility to reclaim a license from a user. Configure this property using the –allowLicenseReclaim command line argument when you run the license server manager (lmadmin).

Three-Server Redundancy Group Information

If you configured the license server for three-server redundancy, this section contains information about the configuration. See the License Administration Guide for information about three-server redundancy.

| • | Quorum State: This is the state of the quorum. As the license server starts up and attempts to establish a quorum, the following states are set in the order listed:

| • | None: The license server is not configured for three-server redundancy.

| • | Initialize: A quorum is being initialized.

| • | Wait: The initialization phase is complete, but a quorum has not yet been established.

| • | Confirm: The license server is waiting for a confirmation message from at least one other license server before the quorum is established.

| • | Up: At least two license servers have established a quorum.

| • | Master: The host name of the Master.

| • | Heartbeat Interval: The value of the HEARTBEAT_INTERVAL attribute defined in the license file.

| • | Primary Is Master: Either true or false, indicating whether the PRIMARY_IS_MASTER attribute is defined in the license file.

| • | Group Member Host: The host names of the three systems that are configured in the license file.

| • | Port: Port number of each system displayed in Group Member Host column.

| • | Status: Status of each system in the Group Member Host column. As each license server joins the quorum, it has one of the following statuses.

| • | None: The license server is not a member of the quorum.

| • | Active: The license server is an active member of the quorum.

| • | Connected: The license server has connected to the quorum.

| • | Connection Failed: The license server attempted to connect to another license server, but it failed.

| • | In Process: The license server is attempting to connect with another license server to establish a quorum.

| • | Initialize: The license server is being initialized as part of the quorum.

| • | Sent: The license server sent a message to another license server in the quorum.

Open topic with navigation